Enhanced Reality Audio in Interactive Networked

Environments

Vicky Hardman and Marcus Iken

Abstract

The human auditory system has a two-fold function, to act as a receiver for spoken language, and also as an interpreter of the omni-directional environment that the listener is in

(to direct the eyes). The acceptance of a network audio tool depends on both its ability to provide communication between remote participants, and its ability to immerse the listener in a natural auditory environment. The first part of this paper describes the multimedia conferencing piloting activities at UCL, that high-lighted the requirement for improved and more natural audio. The

Robust-Audio tool was initially developed to address problems with speech intelligibility, that stem from the use of low-cost shared networks, and general purpose hardware. Recent developments in RAT have addressed the second function of the auditory system and provide 3D spatialisation supported by higher bandwidth speech,

1. Introduction

There are many applications for group-based virtual reality systems, such as visualisation, enhanced reality multimedia conferencing, and entertainment systems. These applications use sound localisation to enhance the presence in the artificial world. Current group-based virtual reality systems use high quality, high bandwidth audio, with specialist hardware to provide 3D spatial audio. If this technology is to mature quickly, then the cost (network bandwidth and computing power) must be reduced, and the systems tested by many simultaneous users on a global basis.

In contrast, the approach presented in this paper is based on the Mbone (the multicast backbone overlay on top of the Internet), which is a multi-way global network that is used to carry multimedia traffic. A variety of multimedia conferencing tools have been developed by various research projects to assess the usability of solutions to the low-cost requirements. Evaluation results from application trials are used to focus new research. Our experience shows that audio is the most important media, in terms of effective communication, and the one with the biggest problems. The audio problems identified so far include, sensitivity to network packet loss, gaps in the audio caused by the lack of real-time support on general purpose hosts, poor hands-free operation, restricted speech intelligibility, and lack of distance cues for speakers.

The Robust-Audio Tool (RAT) is a multi-way multimedia conferencing audio tool that has recently been developed in the Computer Science Department, UCL. RAT offers benefits over most other available audio tools, since it provides packet loss protection, and a mechanism that copes with the lack of real-time support found on most general purpose computing facilities. RAT also offers improved hands-free operation.

Recent work at UCL has begun to address problems such as restricted intelligibility, and the lack of distance cues. The ability to perform real-time 3D audio spatialisation has been added into RAT without any extra specialist hardware. In conjunction, a wideband speech coding algorithm, suitable for use over packet networks, is also being developed for RAT, which will be used to minimise the network bandwidth required by 3D audio. The latest developments begin to address some of the remaining audio problems in multimedia conferences, and produce an audio tool which is suitable for use in virtual reality environments. The recent ability of general purpose computing facilities to support this level of computation, and the emergence of the Mbone as a useable multi-way multimedia network means that virtual reality systems can begin to be realised with low-cost hardware, and evaluated on a large scale.

This work stems from multimedia conferencing piloting applications, such as project MICE[1]

(Multimedia Integrated Conferencing for Europe, and its follow-on Project MERCI - ESPRIT), project

ReLaTe[2] (Remote Language Teaching over SuperJANET - BT/JISC, and its follow-on ReLaTe/2 -

JISC), and more recently the RAT project[3] (EPSRC). Virtual reality work at UCL includes projects such as COVEN[4], and DEVRL[5]. We envisage the possible integration of RAT into Coven.

Some background is given in the first section, which discusses the applications projects in the department. The second section discusses the evaluation results relating to audio, and identifies possible improvements. The third section of the paper briefly discusses the RAT architecture, and highlights some of the recent developments, which improve the quality of the audio over the network, and on the host platform. The fourth section concentrates on the implementation of sound localisation in RAT.

2. Networked Virtual and Enhanced Reality Applications

Networked virtual and enhanced reality applications all have one thing in common; the requirement to communicate over a network in a manner similar to that used in the face-to-face situation.

The applications include the following:

· enhanced reality multimedia conferencing [6][7][8]

· information visualisation (VR-VIBE[9])

Multimedia conferencing is the technology that under-pins many of the new virtual and enhanced reality applications, and it comprises audio, video and shared workspace. Of the three media, audio is still the most important means of communication.

2.1 Multimedia Conferencing

The emergence of a global low-cost shared network - the Mbone - has meant that multimedia conferencing applications are beginning to migrate from the research environment into the commercial world. A strategy of restricting costs enables a critical mass of users to be established, which allows the technology to mature through design iterations and improvements. Low cost multimedia conferencing solutions can only be achieved by using human perception techniques to focus precious computing resources, for example; image rendering in virtual reality worlds is often of much lower resolution when an object is far away, some audio tools in multimedia conferencing only mix the maximum number of sources that a human can discern.

2.2 Low-cost Network and Platforms

The Mbone provides multi-way communication by using a technique known as multicast [10].

Multicasting enables the transmission of multi-way real-time audio and video communication to interested participants, without having to use either complicated set-up procedures (circuits), or consume large amounts of bandwidth (broadcast). The network nodes contrive to transmit only to interested receivers

(figure 1).

Figure 1: Multicast Transmission over the Mbone

The Mbone is a shared heterogenous network, where information is transmitted in packets.

Communication is usually on a `best-effort´ basis, which means that there are no quality of service guarantees (the ability to perform resource reservation is currently being incrementally deployed[11]). The heterogenous nature of the Internet and Mbone has meant rapid global deployment, and cheap network access charges.

The availability of general purpose hosts, such as UNIX-based workstations, and more recently multimedia personal computers, is another factor in the low-cost strategy that promotes a critical mass of users. This is especially true if extra equipment is kept to a minimum. Multimedia conferencing components are consequently implemented as separate software processes on the multi-tasking operating systems, and the implication is that the host must be able to perform real-time compression and delivery

(rendering) of the media in software.

2.3 Multimedia Conferencing Components

Multimedia conferencing over the Mbone provides multiwayaudio, video and shared text

facilities:

· Audio tools , such as vat [12], and RAT [13], enable everyparticipant to hear

everybodyelse in the conference simultaneously. The system interface usually

comprises a window showing a list ofthe participants in the audio conference,

gain and volume controls, power meters to indicate speech activityetc. (Figure

2). In order to talk, the pointer has to be placed in the window, and the left

mouse button pressed. This mechanism is known as `push-to-talk´.

Figure 2: Audio Tool Window

· Video tools , such as vic [14], enable everyparticipant to see video fromevery

other participant (depending on the available bandwidth). Each video image is

displayed in a separate window, and these can be arbitrarilypositioned on the

screen.

· Shared text and whiteboard tools , such as wb [15], and nt [16] enable each

participant to see and edit the same text (wb and nt) and images (wb). Text and

drawings can be entered via the mouse and keyboard, and each participant draws

in a separate colour. Previously stored postscript files can also be imported.

2.4 Business Meeting and Distance Learning Applications

Real applications are currently being piloted over the Mbone, such as business meetings [1], and

distance learning trials [2][1], using audio, video and shared text tools. The ReLaTe project is trialing

remote language teaching over the Mbone, using the tools RAT [13], vic [14], and wb [15] / nt [16], and

has produced an integrated interface for novice computer users (figure 3). Integration of audio and video

information was achieved by using a conference bus, rather than a more conventional method of inter-

process communication. A conference bus transmits multicast information using a ttl of zero, which

retains all the benefits of multicast - multi-way communication, and dynamic group membership - while

restricting the traffic inside the workstation [17].

Figure 3: The ReLaTe Interface

2.5 Trial Observations

Informal evaluation in the MICE project identified audio as the most important medium. This was borne out by formal evaluation during the ReLaTe project, from language teachers, HCI and technical experts, which also identified poor audio quality as being the major problem with the system. A detailed description of the evaluation can be found in [18].

3. Networked Enhanced Reality Audio

Audio was identified early on in the ReLaTe project as being the primary area of concern. The problem can be broken into a number of symptoms that are true of most Mbone multimedia conferences compared to face-to-face situations:

Audio Gaps

Audio packet loss results in gaps in the output speech, and is verydetrimentalto

speech intelligibilityabove 10% loss. Gaps in the output speech can also occur

because ofthe lack ofreal-time support on generalpurpose operating systems,

such as UNIX; samples have to be regularlyfed to the output device, and a

missed dead line results in a gap.

Lack of Hands-free Operation

The lack ofhands-free operation was due to the use ofthe `push-to-talk´ facility.

Use ofthe `push-to-talk´ mechanismreduced the spontaneityand interactivityof

the conversation [18].

Reduced Speech Intelligibility

Restricted speech intelligibilityofan isolated speaker is a result ofusing telephone

qualityspeech. Monauralhearing reduces the intelligibilityofa speaker when

another person speaks (cocktail party effect [19]).

Speaker Identification Difficult

Speaker identification is difficult in most audio tools, since a listener has to look

down the list ofparticipants for a high-lighted name (see figure 2). The ReLaTe

system(figure 3) improved the situation substantiallybyassociating individual

audio power meters with video images, but this technique is still artificial.

Lack of Distance Cues

The audio channelprovided byexisting audio tools sounds acoustically`dead´,

since there are no distance clues in the audio; speech is provided over head-

phones, and the audio sounds as ifit is coming from inside the head. The lack of

distance clues means that some speakers tend to shout, while others speak quietly.

RAT has been developed as a platform for multicast audio research, and the intention is to address

the problems identified above.

Mechanisms to repair packet loss over the network, and to cope with the lack of real-time support

on general purpose operating systems have been developed at UCL [20][21], and initial investigations

show that significant success has been attained. The lack of hands-free operation has also been addressed

by the development of an improved silence detection mechanism. Further work in all of these areas is

planned under Project RAT [3].

It is well known that wide-band speech (16kHz, rather than 8kHz sampling rate) provides greater

speaker intelligibility, and retains more of the individual characteristics of a voice, which allows easier

participant identification. A reduced complexity wide-band speech codec [22] is being developed for RAT

as part of an MRES project at UCL.

Sound localisation [8] has the ability to both position sound sources out in space (which facilitates

easier participant identification), and provide some distance information (which will allow a speaker to

subconsciously determine how loudly to speak). Sound localisation is usually provided in both multimedia

conferencing systems and virtual reality systems by special purpose hardware, such as the convolvatron

[23] and beachtron [24] cards. The DSP-based hardware has the processing power to artificially convert a

mono sound source into localised sound using the Head Related Transfer Functions (HRTF - [25]), and

reverberation [8]. HRTFs simulate the inter-aural intensity and phase differences of sound arriving at the

two ears, together with the effect of head shadows, the effect of the shoulders, and reflections from the

pinnae [23]. In order to successfully externalise the sound, a minimum sampling frequency of 16-32kHz is

required [25]. Uncompressed transmission of this bandwidth would result in excessive network bandwidth

consumption, which should be avoided if at all possible. The 16kHz wide-band speech compression

algorithm [22] can be used to support sound localisation, and the algorithm produces an output bit-rate of

64kbps, which is suitable for transmission over the Mbone. The codec has not been developed for use over

packet networks, but current work at UCL is investigating this problem. The codec provides good enough

quality audio for use with sound localisation techniques. The provision of sound localisation via the

HRTFs in RAT is being developed at UCL.

In the telephone network, distance cues are provided to a speaker by the use of side-tone[26]

(leakage between the microphone and loudspeaker). The provision of side-tone and automatic gain control

[27] are also being developed for RAT.

4. A Robust-Audio Tool

The robust-audio tool (RAT) emerged at UCL as a result of experiences gained from applications

piloting activities (projects MICE and ReLaTe). RAT is based on existing audio tools, such as vat [12],

but it also includes new techniques developed at UCL which improve the quality of the audio. RAT is

currently available for a wide range of platforms: SunOS, Solaris, IRIX, and Win95, and is currently

being ported to HP, DEC Alpha, Linux, and FreeBSD.

A block diagram of RAT can be seen in the diagram (figure 4). The audio tool has been designed

for use with either headsets or a microphone and loudspeaker. At the transmitter, speech samples collected

from the microphone are used to fill a packet, which is then transmitted over the network. At the receiver,

the samples are retrieved from the packet, and sent to the audio device driver, where they are played out to

the headphones or loudspeaker.

Figure 4: Block diagram of RAT

4.1 Silence Detection

Silence detection [27] is commonly used in packet network speech systems to reduce the bandwidth

consumed. Silence is not transmitted, and since at least half of speech is `silence´, this represents a

significant saving. In a multi-way environment, usually only one person is speaking at once, and silence

detection then has the potential to reduce the bandwidth consumed to approximately half of one normal

telephone channel. Silence detection has implications for 3D spatial audio, since if only one person is

speaking at once, then only one sound source needs to be manipulated. Work at UCL as part of the RAT

project will improve the quality of the silence detection algorithm.

4.2 Real-Time Protocol (RTP)

Real-Time Protocol (RTP) was developed for the transmission of real-time audio and video over the

Mbone[28]. RTP provides facilities such as time-stamping, session control etc. Initial proposals from

others at UCL, to develop networked distributed virtual reality protocols for use in a shared multicast

environment propose the use of RTP, and can be found in [29].

4.3 Speech Compression

Speech compression algorithms are used to reduce the packet rate, which improves the packet loss

rate. Existing audio tools transmit telephone quality speech (8kHz sampling rate). 16kHz sampled speech

can be coded using the wide-band coding algorithm [22], and the bandwidth consumption restricted to

reasonable levels. Wideband speech improves the quality of audio, such that individual speakers can be

recognised. The sampling rate offered by wideband speech (16kHz) is also the minimum that is required

in order to externalise 3D sound [25].

4.4 Packet Loss

Packets may be lost over the network, since routers throw away packets when they get congested.

The impact of packet loss on speech quality can be very severe, especially given the packet sizes

commonly used over the Mbone [20]. Work at UCL as part of the RAT project [3] is developing

techniques to improve packet loss robustness. Speech from existing audio tools is intelligible for packet

loss up to 10%, whereas from RAT it is intelligible for up to 30% [13].

4.5 Packet Loss Robustness in RAT

At high loss rates, and for the length of packets commonly used over the Mbone, packet loss can

only be successfully repaired by the use of redundancy [20]. Redundancy transmits a low bandwidth

synthetic version of the speech on the packet behind, which can be used in the event of single packet loss

to repair the speech at the receiver (figure 5).

Figure 5: Redundancy for the audio is carried in the packet behind

This mechanism provides satisfactory speech quality for up to 30% loss (figure 6).

Figure 6: Subjective Assessment of Packet Loss Repaired Using Redundancy

1

2

3

4

5

0% 5% 10% 15% 20% 25% 30% 35% 40% 45% 50% Packet loss

Mean opinion score

No redundancy Redundancy

Bursts of packet loss can be repaired by using multiple copies of redundancy, although what is

really required is to reduce the offered load on the network, by increasing the compression level [20]. This

work is currently being accomplished under Project RAT [3].

4.6 Adaptive Workstation Real-time Performance Management

The lack of support for real-time applications on general purpose computers may produce gaps in

the output audio. In RAT, the adaptive cushion algorithm [21] estimates the current work-load of the host,

and uses the device driver buffer to minimise the occurrence of gaps in the audio, while minimising the

delay. The results show both a decrease in the number and length of audio gaps, and a decrease in the

mean and variance of the perceived end-to-end delay, compared to existing audio tools.

5. Networked 3D Spatial Audio

Networks usually only transmit one channel at low bandwidth to minimise costs. A monaural

signal is known to affect many aspects of the perception of audio (such as speaker identification difficult,

and the lack of distance cues). The provision of natural two channel sound is obviously desirable.

5.1 3D Audio

A mono signal can be transformed into an apparently spatial sound source, by duplicating the

mono signal, and then manipulating the two channels individually to simulate spatialised sound.

Intuitively, one might think that free-field loudspeakers could be used to provide 3D sound, but the

problems of cross-talk (signals from the left loudspeaker reaching the right ear and vice versa), make this

problem more complex (cross-talk cancellation algorithms are required) than when using headsets. In

contrast, cross-talk is not a problem for headsets, but the use of head-tracking devices is still required, or

else the location of a sound object does not change position relative to the user´s head. In multimedia

conferencing, headsets are commonly used with audio tools, such as RAT, to ease problems with hands-

free operation, and so the following descriptions apply to the use of headsets only.

There have been two approaches to providing spatialised audio: lateralisation and localisation.

Lateralisation

Speech based on mono signals is perceived as originating fromthe midpoint

between the two ears, and usuallymore at the back ofthe head. Lateralisation

separates conference participants out in space, although allthe sounds appear to

still come from inside the head.

To achieve pure lateralisation, the application ofthe duplex theory[30] is

sufficient; the channelbeing sent to the far ear has to experience a delayand a

dampening ofthe amplitude relative to the channelbeing sent to the near ear

(figure 7).

Figure 7: Lateralisation from a mono input channel.

However, this simple approach to lateralisation does not take into account the

frequency dependency of the duplex cues.

Localization

Localization aims to transformthe incoming signal in a waythat is faithfulto the

real life situation; this is what the head-related transfer function (HRTF) does

[25], and since sampled speech is a sequence ofimpulses, it can be spatialised by

convolving the HRTF data set with the input audio.

Figure 8: Using the HRTF data sets to produce Localisation.

In contrast to the operations necessaryfor achieving mere lateralisation,

convolutions are costlyin terms ofcomputing resources. In the time domain the

complexity is O(n*m), in the frequency domain O(n*log2n).

5.2 RAT and 3D Audio

Sound localisation is being developed for RAT in order to address a number of problems identified

during ReLaTe [2] and MICE [1] trials. The environment that this system has to work in means that

localisation blur [25] is not as critical as externalising the sound, since we wish to provide a natural

acoustic environment for conference participants, and improve the intelligibility of what is being said, by

separating the sources out in space. Maintaining the low-cost strategy employed in these projects,

necessarily involves making some compromises in the 3D system design. The performance of the

enhanced RAT audio system will be reduced compared to that achievable using dedicated hardware, but

we intend to back up this development with extensive human perception analysis, in order to provide a

system that is adequate for the requirements of multi-way networked enhanced reality multimedia

conferencing.

The low-cost constraints of this development are as follows:

· real-time processing on modern generalpurpose multi-tasking operating systems

(no DSP boards or separate special-purpose hardware)

· minimal use of computing power (other multimedia tools need processor time)

· minimalnetwork bandwidth (currentlythis means using low sampling rates, 16

kHz instead of 32kHz)

As can be seen from the above, the criteria for a low-cost solution are different from the goals

pursued in current VR and perceptual psychology research, where highly accurate localisation is sought

[23]. Within our low-cost strategy, the desired improvement is a qualitative step from a mono signal being

perceived inside the head to externalised sound appearing outside the head, and with reasonable azimuth

separation. The externalisation is further helped in scenarios that include the visual as well as the auditory

sense, as is the case in multimedia conferencing. Visual awareness of the apparent sound sources (i.e.

conference participants) improves externalisation, and reduces the occurrence of front/back reversals [31].

In the light of the different circumstances and objectives compared to mainstream virtual reality

research, a low-cost strategy for the general design of the module can be pursued.

5.2.1 Design and Implementation

Localisation is known to consist of two classes of effects: diffractions caused by the upper torso,

and the duplex cues [31]. The HRTF data set [32] was empirically measured, and therefore includes both

of these effects. Analysis of the HRIR (impulse responses) shows that the delay and attenuation of the

signal can be identified. Since convolution is very costly in terms of computing power, complexity

reduction techniques were sought for implementation in RAT.

In the RAT 3D spatialaudio system, the HRTF transformation has been split up into two

distinctive stages:

· effects that are not present in the pure mono signal, but make the signalappear to

have been transferred from the free-field to the eardrum

· duplex cues, i.e. delay and gain

Figure 9: Use of the HRTF Data Set in RAT

Figure 9 shows that the first stage is a convolution with an HRTF data set which results in the

externalization of the signal. The second stage implements the duplex cues (lateralisation). Since the delay and gain operations consume negligible processing power compared to the convolution, this design

requires roughly half the computational power that would be used in the approach outlined in Figure 8.

This would be well within the real-time capabilities of general purpose workstations.

The RAT architecture has been designed to allow relatively painless enhancement. Figure 10

illustrates the integration of the sound localisation module into RAT.

Figure 10: The Integration of 3D Audio into RAT

Upon joining a multicast group, each participant is assigned an azimuth on the horizontal. Using

the relevant HRTF data set for that azimuth, appropriate delay and gain values are calculated. After the

received packets are buffered and decoded, the speech samples are convolved with a chosen data set, and

the result replicated. The far ear samples are then multiplied with the gain factor (IID), and delayed by a

number of samples equivalent to the calculated delay (IDT).

5.2.2 Selection and Preparation of HRTF Data Sets

Due to the enormous amount of work needed to measure an adequate number of related HRTF data

sets, only one has so far been released into the public domain (data recorded at MIT using a KEMAR

dummy [32]), although others exist [25]. The MIT data set was recorded at a sampling rate of 44.1kHz,

and two versions are provided: the recorded sets and the diffuse field sets. The recorded data sets contain

some unwanted components: inaccuracies of the measurement set-up, and most importantly, the ear-canal

response. Using headsets means that an ear-canal response will be included naturally, so the diffuse-field

version must be used instead.

The data sets were re-sampled to 16 kHz using a program based on the sinc-pulse function to

restore the continuous time signal [33]. This reduces the filter length from 512 values to (512 * 16/44.1 =)

185 values. Using the fact that the 64 most significant values of a 512 value data set produce nearly the

same frequency response as the complete set [Begault], the (64 * 16/44.1 =) 24 most relevant values are

extracted from the 185 resulting from the resampling operation.

In the implementation of this operation in RAT, we use a sliding window to isolate each possible

combination of 24 consecutive taps, and sum the absolute values. The greatest resulting value is taken to

mean that we have identified the `good taps´ [31] in each filter. This is done for both data sets relating to

a particular azimuth. The next state is to identify the delay and gain cues from the two filters. This is achieved by calculating the delay from the separation between the `good taps´ for each filter, and by

evaluating the power of near ear divided by the power of far ear to give the gain.

5.2.3 Preliminary Results

The RAT interface was enhanced to allow the user to switch between monaural sound, and filtered

binaural sound. Preliminary informal listening tests revealed that listeners were able to report

externalisation of the sound source. Plots of the frequency responses of the near ear HRTF data sets at

44.1kHz and 16kHz can be seen below.

Figure 11: Comparison of the Frequency Responses of an HRTF Data Set Used in RAT, sampled at 16kHz

with identification of 32 `Good Taps´ to the original data set, sampled at 44.1 kHz and 512 taps.

The graph (figure 11) shows that down-sampling and extracting a sub-set of significant taps does

not affect the general shape of the frequency response.

6. Conclusion

The paper has shown approaches to solve audio problems that invariably appear with multimedia

conferences over `shared´ networks, and that use only general purpose hardware. The approaches

described will provide higher acceptance of an audio tool like RAT, because they address the two main

functions of the human auditory system.

Solutions were presented that tackle the problems of audio, such as gaps in the output stream

(resulting from packet loss and the lack of real-time support on general purpose operating systems), and

the lack of hands-free operation, that initially proved to be such problems for our applications piloting

projects. These solutions now provide a greater robustness to the audio output, and therefore to the

communication between remote participants.

Later evaluation of the piloting projects, identified further potential areas of improvement,

specifically providing a more immersive environment. The techniques researched and integrated into RAT

employ some novel complexity reduction methods that enable real-time operation in a multi-tasking

environment, using exclusively general purpose hardware.

7. Future Work

The success of the pre-split HRTF design as outlined in section 5.2.1. crucially depends on the

quality of the data set applied. The use of a down-sampled individual data set can only be regarded as a

starting point.

Work in the near future will comprise:

· the use ofgeneralised HRTF data that exploits the common features ofindividual

data sets.

· informal`playing´ with the data sets accompanied byhuman perception

evaluation with regards to the externalisation and reverberation achieved.

Work in the medium future might include the implementation of proper distance cues (ratio of

direct to reverberation signals and dampening of high frequency components).

Acknowledgments

We would like to acknowledge the following, who work together to develop RAT using a wide varietyof backgrounds

and specialist knowledge:Angela, Isidor, Anna, Colin, Orion, Mark, Jon, and Peter. We would also like to

acknowledge Isidor, Anna, Mel and Anthony for their comments on this paper.

Biographies

VickyHardman is a newlyappointed lecturer in the Multimedia Group, Department of Computer Science, UCL. She

has worked on a number of national and international research projects in multimedia conferencing, such as ReLaTe

(BT/JISC - where she was the research fellow on the project), MICE (ESPRIT - which pilots multimedia conferencing

systems), and Unison (ALVEY - which developed a multimedia packet network). Recently, she has been made co-

investigator of the continuation of the ReLaTe project (JISC), and co-investigator of an EPSRC project (RAT

#GR/K72780). Current research areas are speech over packet networks, and enhanced realitysystems for use in

multicast packet networks. Vickyhas a PhD in Speech over Packet Networks, from Department of Electronic and

Electrical Engineering, Loughborough Universityof Technology. She has also worked for voice switching

manufacturers for 3 years, on CCS7 and CAS voice networks.

Marcus Iken is a final year student at Stuttgart University. He is currentlyundertaking his final year research project

at UCL with Vicky Hardman. Marcus hopes to study a PhD at UCL in sound localisation.

References

[1]HandleyM.,Kirstein P.,Sasse M.A., `Multimedia Integrated Conferencing for European Researchers (MICE):

piloting activities´ Computer Networks and ISDN Systems,26(3),275-290, 1995.

[2] Buckett J. Campbell I. Watson T.J. Sasse M.A. Hardman V.J. Watson A. `ReLaTe:Remote Language Teaching

over SuperJANET´ Proceedings of UKERNA 95, Networkshop, March 1995.

[3] `Multi-wayMulticast Speech for Multimedia Conferencing over Heterogenous Shared Packet Networks (RAT

Robust-Audio Tool)´, EPSRC Research Grant #GR/K72780.

[4] `Coven: Collaborative Virtual Environments´, ACTS 4th Framework Project.

[5] `DEVRL: Distributed Extensible Virtual Reality´ EPSRC:ROPA Project #AC040.

[6] Hardman V.J., `Low-cost Multi-way Distance Learning´ Proceedings of the Coseners Network Shop, 1996.

[7] Yngvesson J., Kvarnstrom B., `Telepresens in Conference Applications´ MultiG Workshop 1992.

[8] Strauss, Blauert J., `Virtual AuditoryEnvironments´, Proceedings of the Conference of the FIVE Working Group

(ESPRIT 9122), QMW, University of London, 18-19 December 1995.

[9] Benford, S., Snowdon D., Greenhalgh C., Ingram R., Knox I., Brown C., `VR-VIBE:AVirtual Environment for

Co-operative Information Retrieval´ Eurographics 95, Publ. Blackwell.

[10] Deering S., `Host Exetensions for IP Multicasting. Request for comments RFC 1112, Internet Engineering Task

Force, August 1989.

[11] Zhang L., Deering S., Estrin D., Shenker S., Zappala D.,´RSVP:Anew Resource Reservation Protocol´, IEEE

Net, Sept. 1993., Volume 7., No. 5, pp.8-18.

[12] Jacobson V. `VAT manual pages´, Lawrence Berkeley Laboratory (LBL) February 1992.

[13] Hardman V., Kouvelas I., Sasse M.A., Watson A., `APacket Loss Robust-Audio Tool for Use over the Mbone´

Department of Computer Science Research Note, RN/96/8

[14]McCanne S., Jacobsen V., `Vic:AFlexible Framework for Packet Video. Proceedings of ACM Multimedia `95,

November 1995.´

[15]McCanne S., `ADistributed Whiteboard for Network Conferencing´, May1992, UC BerkeleyCS 268 Computer

Networks term Project.

[16] Handley M., `A Shared Text Editor´ URL: http://www.cs.ucl.ac.uk/mice/mice_home.html

[17] HandleyM.J., Wakeman I., `CCCP:Conference Control Channel Protocol, AScaleable Base for Building

Conference Control Applications´ Conference Proceedings ACM SIGCOMM95, Cambridge Massachusetts, 1995.

[18] Watson A., Sasse M.A., `Evaluating Audio and Video Qualityin Multimedia Conferencing Systems´ To appear

in Interacting with Computers Journal.

[19] CherryC.E., `Some Experiemnts on the Recognition of Speech, with One and Two Ears´ Journal of the

Acoustical Society of America, Vol. 25, No. %, pp. 975-979, USA.

[20] Hardman V., Sasse M.A., HandleyM., Watson A., `Robust Audio for Use over the Internet´, INET 95, Honalulu,

Oahu, Hawaii, June 1995.

[21] Kouvelas, I., Hardman V.J.´Overcoming Workstation Scheduling Problems in a Real-Time Audio Tool´ Dept.

Computer Science, UCL, Research Note No. RN/96/44.

[22] Hardman V.J., `Wide-band Speech Teleconferencingover an Integrated Network´, PhD Thesis, Dept. Electronic

and Electrical Engineering, Loughborough University of Technology, Loughborough, Leicestershire, November 1993.

[23] Wenzel E.M.`Localisation in Virtual Acoustic Displays´ Published in Presence,Volume1,Number 1, pp80 - 107.

[24] `Beachtron Card: Crystal River Engineering´, URL http://www.cre.com/index.html

[25] Wightman F.L, Kistler D.J., `Headphone Simulation of Free-Field Listening. I:Stimulus Synthesis´ Journal of

the Acoustical Socity of America, Vol. 85, No. 2, 1989, pp. 858-867, USA.

[26] Richards D.L.´ Telecommunication by Speech´ Pub. Butterworth and Co. 1973.

[27] Rabiner L.R., Schafer R.W., `Digital processing of Speech Signals´ Publ. Prentice Hall, 1978.

[28] `RTP: A Transport Protocol for Real-Time Applications´, Audio-Video Transport WG, rfc 1889.

[29] Crowcroft J., HandleyM., `Network Support for Scaleable Distributed MultipartyVirtual Reality´ Conference

EPFL-UCB, Workshop on Multimedia Networking 96, Lausanne, Switzerland, July 11-12, 1996.

[30] Blauert J., `Spatial Hearing, The Psychophysics of Human Sound Localisation´, The MIT Press, Massachusetts,

USA, 1983.

[31] Begault D.R. `3D Sound for Virtual Reality and Multimedia´ Published by Academic Press, 1994.

[32] Gardner B., Martin K., `HRTF Measurements of a KEMAR Dummy-head Microphone´ Technical Paper No.

280, MIT Media Lab. Perceptual Computing, Dept. Electrical Engineering and Computer Science, USA, 1994.

[33] Van Den Enden A.W.M., Verhoeckx N.A.M.´Discrete Signal Processing - An Introduction´, Pub. Prentice Hall,

1989.